-------------------------------------------------------------
 MARPLE: Model for Assignment and Regional PoLicy Evaluation 
 The version used is: MARPLE 3.9.0 of 18-07-2025
 Copyright (c) 2004-2023, Henk Taale, Rijkswaterstaat and    
                          Delft University of Technology     
-------------------------------------------------------------

Date and time of starting the run is: 18-Jul-2025 16:37:45

The file with simulation parameters is: 
C:\Onderhoud Applicaties\MARPLEinstall\Example\MARPLEparm.txt

The file with network input is: 
C:\Onderhoud Applicaties\MARPLEinstall\Example\Example-Network.txt

The output file is: 
C:\Onderhoud Applicaties\MARPLEinstall\Example\Example-Output.txt


MARPLE parameters:

//General
;Assign Optimization Metering SmoothG SmoothFlow DelayType InitialFlow ThresFlow ConvError minCounter maxCounter
    2        0           1        0       1          0          1          0        1.000        1         30

//Assignment
;VI-rho CF-beta CF-gamma Kirchhoff initialAssign MobScan
  10.00    1.00     2.00         0             1       0 

//LocalControl
;LContrMethod LOptPeriod
        1         60 

//AntControl
;nrAssign nRTperiods optCriterium LTimeStepOpt
        2          1            2          150 

//Routes
;nrRoutes nrRand scaleFac linkCost linkEqual junctionDelay ODdist 
     4       60    0.66       1      1.00              0        1  

//VehPar
;VehLen TruckV minV1 MinV2  Ja1  Ja2  Ja3  Ja4  Ja5  Ja6  Ja7  Ja8  Ja9 
   7.5     80    10    10    85   75   60   50   40   20   15   10   10 

//TollPar
;TollType ValTime1  ValTime2  ValTime3  ValTime4 
     1       10.00     15.00      8.50     24.60  

//EventSimPar
;EventSimType  EventSimAssign  EventSimNrIter 
     0                 2                 3  

//TimePenaltyPar
;TimePenaltyType  IC-threshold 
     0                95.0                

//Output
;OutputType  Binary  Emissions 
          4       1       1 


//Resume
;ResumeSim 
      0


-----------------------------------
 Network characteristics
-----------------------------------
Number of links        :         13
Number of short links  :          0
Number of nodes        :         11
Number of origins      :          2
Number of destinations :          2
Number of OD pairs     :          3
Number of routes       :          4
-----------------------------------


Network input parameters:
-------------------------

//Parameters 
;nrTimePeriods LengthTim LTimeStep ScaleFlow ScaleCap ScaleSpeed DemandPar 
             7       900        20    1.0000   1.0000     1.0000         0

//Events 
;begintime endtime linknr nrlanes satflow   vfree  type 
                                      (%)     (%) 
       900    1500      4      -1      50      70     1

//UserClasses 
;userclass percentage teta penalty 
         1      20.00  0.0     0.0
         2      40.00  1.0     0.0
         3      40.00  3.0     0.0

Total number of links too short for the length of the timestep:    0


Output for iterations:
----------------------

//LinkOutput (after the first simulation)
------------------------------------------------------------------------------------------------------
       period|      linknr|  link length|   density|   speed| std speed|    inflow|   outflow|   queue|
             |            |      (m)    |(veh/km.l)| (km/hr)|   (km/hr)|  (veh/hr)|  (veh/hr)|     (m)|
-------------|------------|-------------|----------|--------|----------|----------|----------|--------|
            1            1          2713     14.188   114.55       0.00    3405.00    3405.00        0  
            1            2           670     13.563   115.55       0.00    3255.00    3255.00        0  
            1            3          2045     14.506   113.48       0.38    3588.33    3609.63        0  
            1            4          1046     15.129   106.38       4.50    3942.96    3968.52        0  
            1            5           500     55.544    12.94       7.20     525.00     333.33      184  
            1            6          1654      6.563    79.69       0.00     525.00     525.00        0  
            1            7           500     55.544    12.94       7.20     525.00     333.33      184  
            1            8           715      6.562    79.69       0.00     525.00     525.00        0  
            1            9           702      2.143    32.29       0.00     150.00     150.00        0  
            1           11           999      7.500    69.52       0.00    1050.00    1050.00        0  
            1           12           570      2.143    69.90       0.00     150.00     150.00        0  
            1           13           400      7.500    31.57       0.00     525.00     525.00        0  
            1           14           400      7.500    26.31       0.00     525.00     525.00        0  
            2            1          2713     19.439    86.73       4.24    4190.00    4067.89        0  
            2            2           670     20.735    95.48      11.32    3874.27    3812.11       11  
            2            3          2045     76.301    37.39      23.82    4145.44    2522.67      802  
            2            4          1046     27.083    53.88      22.01    2856.00    2790.16       95  
            2            5           500    126.328    10.00       0.00     387.80     333.33      456  
            2            6          1654     29.216    52.79      20.11     750.87     387.80      248  
            2            7           500    126.266    10.00       0.00     387.80     333.33      456  
            2            8           715     35.890    48.41      22.86     600.72     387.80      152  
            2            9           702      3.998    31.44       0.33     193.61     187.23        0  
            2           11           999     10.757    69.12       0.06    1575.00    1548.41        0  
            2           12           570      2.660    69.87       0.02     187.23     185.63        0  
            2           13           400     20.859    27.71       0.97     774.21     750.87        0  
            2           14           400     62.187    14.34       5.89     774.21     600.72      115  
            3            1          2713     17.986   106.49       3.11    3875.00    3917.00        0  
            3            2           670     17.783   102.65      13.57    3715.19    3766.79        8  
            3            3          2045    120.180    18.49       0.61    4100.12    3950.67     1445  
            3            4          1046     22.752    85.00       0.00    4284.00    4284.00        0  
            3            5           500    129.630    10.00       0.00     333.33     333.33      472  
            3            6          1654     91.022    19.00       3.29     735.46     333.33     1047  
            3            7           500    129.630    10.00       0.00     333.33     333.33      472  
            3            8           715    118.619    14.87       2.27     475.57     333.33      608  
            3            9           702      4.504    31.25       0.10     201.81     201.81        0  
            3           11           999      8.226    67.57       1.80    1260.00    1274.81        6  
            3           12           570      2.709    69.86       0.00     201.81     202.34        0  
            3           13           400     24.533    26.36       4.15     778.80     735.46        9  
            3           14           400    126.459    10.00       0.00     496.01     475.57      352  
            4            1          2713     14.142   115.39       1.29    3250.00    3335.78        0  
            4            2           670     13.530   115.16       2.26    3231.34    3244.61        0  
            4            3          2045    114.047    17.64       0.31    3577.94    3934.00     1568  
            4            4          1046     22.752    85.00       0.00    4284.00    4284.00        0  
            4            5           500    129.444    10.00       0.00     349.63     350.00      465  
            4            6          1654    131.585    13.19       0.61     415.37     349.63     1580  
            4            7           500    129.630    10.00       0.00     333.33     333.33      472  
            4            8           715    130.743    13.05       0.00     333.33     333.33      687  
            4            9           702      1.074    33.16       0.43     104.43     114.62        0  
            4           11           999     13.146    56.93      11.16    1050.00     875.58       61  
            4           12           570      1.220    69.92       0.03     114.62     118.35        0  
            4           13           400    106.974    11.64       2.54     542.25     415.37      289  
            4           14           400    128.704    10.00       0.00     333.33     333.33      372  
            5            1          2713      7.834   118.46       0.44    2200.00    2340.00        0  
            5            2           670      9.265   118.29       0.88    2234.70    2258.03        0  
            5            3          2045    119.438    16.34       0.97    3343.03    2884.00     1733  
            5            4          1046     22.752    85.00       0.00    4284.00    4284.00        0  
            5            5           500    117.778    18.18       1.61    1376.67    1400.00      215  
            5            6          1654     84.504    23.92       8.85     653.76    1376.67      833  
            5            7           500    113.404    15.83       4.87     951.90    1085.00      245  
            5            8           715     53.320    43.30      25.66     597.63     951.90      215  
            5            9           702      1.001    33.19       0.31     105.30     105.30        0  
            5           11           999      7.370    60.79      13.57     630.00     862.13       42  
            5           12           570      1.093    69.93       0.01     105.30     105.30        0  
            5           13           400     67.409    19.39      10.54     461.59     653.76      139  
            5           14           400     85.395    12.27       4.03     402.70     597.63      210  
            6            1          2713      1.519   119.47       0.14    1150.00    1286.71        0  
            6            2           670      5.124   117.94       4.20    1176.85    1200.18        1  
            6            3          2045     75.327    33.62      27.81    1507.49    3592.24     1124  
            6            4          1046     22.071    86.29       6.06    4133.59    4284.00        0  
            6            5           500     24.167    67.26      19.95     309.30     541.36       61  
            6            6          1654      3.282    77.95       6.38     170.89     309.30        7  
            6            7           500      7.430    74.59      11.72     184.66     307.31       17  
            6            8           715      1.356    79.91       0.04     168.50     184.66        0  
            6            9           702      1.168    33.10       0.57     109.86     109.86        0  
            6           11           999      0.876    69.88       0.02     315.00     322.00        0  
            6           12           570      1.153    69.93       0.02     109.86     109.86        0  
            6           13           400      2.454    36.61       0.43     161.00     170.89        0  
            6           14           400      2.354    32.17       0.52     161.00     168.50        0  
            7            1          2713      1.177   119.49       0.00    1150.00    1150.00        0  
            7            2           670      4.353   119.55       0.00    1050.00    1050.00        0  
            7            3          2045      1.640   119.47       0.00    1207.50    1207.50        0  
            7            4          1046      3.625   119.22       0.98    1365.00    1374.65        0  
            7            5           500      1.750    79.73       0.00     157.50     157.50        0  
            7            6          1654      1.971    79.92       0.00     157.50     157.50        0  
            7            7           500      1.750    79.73       0.00     157.50     157.50        0  
            7            8           715      1.224    79.92       0.00     157.50     157.50        0  
            7            9           702      0.791    33.30       0.00     100.00     100.00        0  
            7           11           999      0.876    69.88       0.00     315.00     315.00        0  
            7           12           570      0.975    69.93       0.00     100.00     100.00        0  
            7           13           400      2.188    36.70       0.00     157.50     157.50        0  
            7           14           400      2.188    32.28       0.00     157.50     157.50        0  
//End---------------------------------------------------------------------------

Total distance travelled for the whole network of the initial simulation is :     38883.24 veh.km
Total distance travelled for network part   1 of the initial simulation is  :     35973.71 veh.km
Total distance travelled for network part   2 of the initial simulation is  :      2909.53 veh.km

Total time spent for the whole network of the initial simulation is         :       881.58 veh.hrs
Total time spent for network part   1 of the initial simulation is          :       783.48 veh.hrs
Total time spent for network part   2 of the initial simulation is          :        98.11 veh.hrs

Average speed for the whole network of the initial simulation is            :        44.11 km.hr
Average speed for network part   1 of the initial simulation is             :        45.92 km.hr
Average speed for network part   2 of the initial simulation is             :        29.66 km.hr

Total toll for the whole network of the initial simulation is               :      3888.32 Euro
Total toll for network part   1 of the initial simulation is                :      3597.37 Euro
Total toll for network part   2 of the initial simulation is                :       290.95 Euro

Total delay for the whole network of the initial simulation is              :       531.51 veh.hrs
Total delay for network part   1 of the initial simulation is               :       474.20 veh.hrs
Total delay for network part   2 of the initial simulation is               :        57.31 veh.hrs

Total entrance delay for the whole network of the initial simulation is     :         0.00 veh.hrs
Total entrance delay for network part   1 of the initial simulation is      :         0.00 veh.hrs
Total entrance delay for network part   2 of the initial simulation is      :         0.00 veh.hrs


Total distance travelled for the whole network of iteration   1 is          :     38860.01 veh.km
Total distance travelled for network part   1 of iteration    1 is          :     35941.34 veh.km
Total distance travelled for network part   2 of iteration    1 is          :      2918.67 veh.km

Total time spent for the whole network of iteration   1 is                  :       849.53 veh.hrs
Total time spent for network part   1 of iteration    1 is                  :       748.91 veh.hrs
Total time spent for network part   2 of iteration    1 is                  :       100.62 veh.hrs

Average speed for the whole network of iteration   1 is                     :        45.74 km.hr
Average speed for network part   1 iteration       1 is                     :        47.99 km.hr
Average speed for network part   2 iteration       1 is                     :        29.01 km.hr

Total delay for the whole network of iteration   1 is                       :       499.58 veh.hrs
Total delay for network part   1 of iteration    1 is                       :       439.87 veh.hrs
Total delay for network part   2 of iteration    1 is                       :        59.71 veh.hrs

Total entrance delay for the whole network of iteration   1 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    1 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    1 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   1 and time period   1 is    :        0.7899
The smooth factor for the flows for iteration   1 and time period   2 is    :        0.7899
The smooth factor for the flows for iteration   1 and time period   3 is    :        0.7899
The smooth factor for the flows for iteration   1 and time period   4 is    :        0.7899
The smooth factor for the flows for iteration   1 and time period   5 is    :        0.7899
The smooth factor for the flows for iteration   1 and time period   6 is    :        0.7899
The smooth factor for the flows for iteration   1 and time period   7 is    :        0.7899

Total distance travelled for the whole network of iteration   2 is          :     38776.56 veh.km
Total distance travelled for network part   1 of iteration    2 is          :     35825.13 veh.km
Total distance travelled for network part   2 of iteration    2 is          :      2951.43 veh.km

Total time spent for the whole network of iteration   2 is                  :       874.39 veh.hrs
Total time spent for network part   1 of iteration    2 is                  :       758.46 veh.hrs
Total time spent for network part   2 of iteration    2 is                  :       115.92 veh.hrs

Average speed for the whole network of iteration   2 is                     :        44.35 km.hr
Average speed for network part   1 iteration       2 is                     :        47.23 km.hr
Average speed for network part   2 iteration       2 is                     :        25.46 km.hr

Total delay for the whole network of iteration   2 is                       :       524.90 veh.hrs
Total delay for network part   1 of iteration    2 is                       :       450.29 veh.hrs
Total delay for network part   2 of iteration    2 is                       :        74.60 veh.hrs

Total entrance delay for the whole network of iteration   2 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    2 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    2 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   2 and time period   1 is    :        0.6012
The smooth factor for the flows for iteration   2 and time period   2 is    :        0.6012
The smooth factor for the flows for iteration   2 and time period   3 is    :        0.6012
The smooth factor for the flows for iteration   2 and time period   4 is    :        0.6012
The smooth factor for the flows for iteration   2 and time period   5 is    :        0.6012
The smooth factor for the flows for iteration   2 and time period   6 is    :        0.6012
The smooth factor for the flows for iteration   2 and time period   7 is    :        0.6012

Total distance travelled for the whole network of iteration   3 is          :     38772.72 veh.km
Total distance travelled for network part   1 of iteration    3 is          :     35817.72 veh.km
Total distance travelled for network part   2 of iteration    3 is          :      2955.01 veh.km

Total time spent for the whole network of iteration   3 is                  :       851.28 veh.hrs
Total time spent for network part   1 of iteration    3 is                  :       743.74 veh.hrs
Total time spent for network part   2 of iteration    3 is                  :       107.55 veh.hrs

Average speed for the whole network of iteration   3 is                     :        45.55 km.hr
Average speed for network part   1 iteration       3 is                     :        48.16 km.hr
Average speed for network part   2 iteration       3 is                     :        27.48 km.hr

Total delay for the whole network of iteration   3 is                       :       501.77 veh.hrs
Total delay for network part   1 of iteration    3 is                       :       435.59 veh.hrs
Total delay for network part   2 of iteration    3 is                       :        66.18 veh.hrs

Total entrance delay for the whole network of iteration   3 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    3 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    3 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   3 and time period   1 is    :        0.4654
The smooth factor for the flows for iteration   3 and time period   2 is    :        0.4654
The smooth factor for the flows for iteration   3 and time period   3 is    :        0.4654
The smooth factor for the flows for iteration   3 and time period   4 is    :        0.4654
The smooth factor for the flows for iteration   3 and time period   5 is    :        0.4654
The smooth factor for the flows for iteration   3 and time period   6 is    :        0.4654
The smooth factor for the flows for iteration   3 and time period   7 is    :        0.4654

Total distance travelled for the whole network of iteration   4 is          :     38763.03 veh.km
Total distance travelled for network part   1 of iteration    4 is          :     35805.02 veh.km
Total distance travelled for network part   2 of iteration    4 is          :      2958.01 veh.km

Total time spent for the whole network of iteration   4 is                  :       872.56 veh.hrs
Total time spent for network part   1 of iteration    4 is                  :       767.69 veh.hrs
Total time spent for network part   2 of iteration    4 is                  :       104.87 veh.hrs

Average speed for the whole network of iteration   4 is                     :        44.42 km.hr
Average speed for network part   1 iteration       4 is                     :        46.64 km.hr
Average speed for network part   2 iteration       4 is                     :        28.21 km.hr

Total delay for the whole network of iteration   4 is                       :       523.12 veh.hrs
Total delay for network part   1 of iteration    4 is                       :       459.65 veh.hrs
Total delay for network part   2 of iteration    4 is                       :        63.47 veh.hrs

Total entrance delay for the whole network of iteration   4 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    4 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    4 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   4 and time period   1 is    :        0.3620
The smooth factor for the flows for iteration   4 and time period   2 is    :        0.3620
The smooth factor for the flows for iteration   4 and time period   3 is    :        0.3620
The smooth factor for the flows for iteration   4 and time period   4 is    :        0.3620
The smooth factor for the flows for iteration   4 and time period   5 is    :        0.3620
The smooth factor for the flows for iteration   4 and time period   6 is    :        0.3620
The smooth factor for the flows for iteration   4 and time period   7 is    :        0.3620

Total distance travelled for the whole network of iteration   5 is          :     38761.76 veh.km
Total distance travelled for network part   1 of iteration    5 is          :     35803.26 veh.km
Total distance travelled for network part   2 of iteration    5 is          :      2958.50 veh.km

Total time spent for the whole network of iteration   5 is                  :       852.26 veh.hrs
Total time spent for network part   1 of iteration    5 is                  :       744.77 veh.hrs
Total time spent for network part   2 of iteration    5 is                  :       107.49 veh.hrs

Average speed for the whole network of iteration   5 is                     :        45.48 km.hr
Average speed for network part   1 iteration       5 is                     :        48.07 km.hr
Average speed for network part   2 iteration       5 is                     :        27.52 km.hr

Total delay for the whole network of iteration   5 is                       :       502.82 veh.hrs
Total delay for network part   1 of iteration    5 is                       :       436.74 veh.hrs
Total delay for network part   2 of iteration    5 is                       :        66.08 veh.hrs

Total entrance delay for the whole network of iteration   5 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    5 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    5 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   5 and time period   1 is    :        0.2822
The smooth factor for the flows for iteration   5 and time period   2 is    :        0.2822
The smooth factor for the flows for iteration   5 and time period   3 is    :        0.2822
The smooth factor for the flows for iteration   5 and time period   4 is    :        0.2822
The smooth factor for the flows for iteration   5 and time period   5 is    :        0.2822
The smooth factor for the flows for iteration   5 and time period   6 is    :        0.2822
The smooth factor for the flows for iteration   5 and time period   7 is    :        0.2822

Total distance travelled for the whole network of iteration   6 is          :     38760.08 veh.km
Total distance travelled for network part   1 of iteration    6 is          :     35800.69 veh.km
Total distance travelled for network part   2 of iteration    6 is          :      2959.39 veh.km

Total time spent for the whole network of iteration   6 is                  :       874.10 veh.hrs
Total time spent for network part   1 of iteration    6 is                  :       767.36 veh.hrs
Total time spent for network part   2 of iteration    6 is                  :       106.74 veh.hrs

Average speed for the whole network of iteration   6 is                     :        44.34 km.hr
Average speed for network part   1 iteration       6 is                     :        46.65 km.hr
Average speed for network part   2 iteration       6 is                     :        27.72 km.hr

Total delay for the whole network of iteration   6 is                       :       524.67 veh.hrs
Total delay for network part   1 of iteration    6 is                       :       459.35 veh.hrs
Total delay for network part   2 of iteration    6 is                       :        65.32 veh.hrs

Total entrance delay for the whole network of iteration   6 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    6 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    6 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   6 and time period   1 is    :        0.2203
The smooth factor for the flows for iteration   6 and time period   2 is    :        0.2203
The smooth factor for the flows for iteration   6 and time period   3 is    :        0.2203
The smooth factor for the flows for iteration   6 and time period   4 is    :        0.2203
The smooth factor for the flows for iteration   6 and time period   5 is    :        0.2203
The smooth factor for the flows for iteration   6 and time period   6 is    :        0.2203
The smooth factor for the flows for iteration   6 and time period   7 is    :        0.2203

Total distance travelled for the whole network of iteration   7 is          :     38758.62 veh.km
Total distance travelled for network part   1 of iteration    7 is          :     35798.75 veh.km
Total distance travelled for network part   2 of iteration    7 is          :      2959.88 veh.km

Total time spent for the whole network of iteration   7 is                  :       853.12 veh.hrs
Total time spent for network part   1 of iteration    7 is                  :       743.81 veh.hrs
Total time spent for network part   2 of iteration    7 is                  :       109.31 veh.hrs

Average speed for the whole network of iteration   7 is                     :        45.43 km.hr
Average speed for network part   1 iteration       7 is                     :        48.13 km.hr
Average speed for network part   2 iteration       7 is                     :        27.08 km.hr

Total delay for the whole network of iteration   7 is                       :       503.70 veh.hrs
Total delay for network part   1 of iteration    7 is                       :       435.82 veh.hrs
Total delay for network part   2 of iteration    7 is                       :        67.89 veh.hrs

Total entrance delay for the whole network of iteration   7 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    7 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    7 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   7 and time period   1 is    :        0.1722
The smooth factor for the flows for iteration   7 and time period   2 is    :        0.1722
The smooth factor for the flows for iteration   7 and time period   3 is    :        0.1722
The smooth factor for the flows for iteration   7 and time period   4 is    :        0.1722
The smooth factor for the flows for iteration   7 and time period   5 is    :        0.1722
The smooth factor for the flows for iteration   7 and time period   6 is    :        0.1722
The smooth factor for the flows for iteration   7 and time period   7 is    :        0.1722

Total distance travelled for the whole network of iteration   8 is          :     38757.98 veh.km
Total distance travelled for network part   1 of iteration    8 is          :     35797.64 veh.km
Total distance travelled for network part   2 of iteration    8 is          :      2960.34 veh.km

Total time spent for the whole network of iteration   8 is                  :       874.28 veh.hrs
Total time spent for network part   1 of iteration    8 is                  :       767.02 veh.hrs
Total time spent for network part   2 of iteration    8 is                  :       107.27 veh.hrs

Average speed for the whole network of iteration   8 is                     :        44.33 km.hr
Average speed for network part   1 iteration       8 is                     :        46.67 km.hr
Average speed for network part   2 iteration       8 is                     :        27.60 km.hr

Total delay for the whole network of iteration   8 is                       :       524.86 veh.hrs
Total delay for network part   1 of iteration    8 is                       :       459.03 veh.hrs
Total delay for network part   2 of iteration    8 is                       :        65.83 veh.hrs

Total entrance delay for the whole network of iteration   8 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    8 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    8 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   8 and time period   1 is    :        0.1348
The smooth factor for the flows for iteration   8 and time period   2 is    :        0.1348
The smooth factor for the flows for iteration   8 and time period   3 is    :        0.1348
The smooth factor for the flows for iteration   8 and time period   4 is    :        0.1348
The smooth factor for the flows for iteration   8 and time period   5 is    :        0.1348
The smooth factor for the flows for iteration   8 and time period   6 is    :        0.1348
The smooth factor for the flows for iteration   8 and time period   7 is    :        0.1348

Total distance travelled for the whole network of iteration   9 is          :     38757.38 veh.km
Total distance travelled for network part   1 of iteration    9 is          :     35796.88 veh.km
Total distance travelled for network part   2 of iteration    9 is          :      2960.51 veh.km

Total time spent for the whole network of iteration   9 is                  :       853.62 veh.hrs
Total time spent for network part   1 of iteration    9 is                  :       744.36 veh.hrs
Total time spent for network part   2 of iteration    9 is                  :       109.25 veh.hrs

Average speed for the whole network of iteration   9 is                     :        45.40 km.hr
Average speed for network part   1 iteration       9 is                     :        48.09 km.hr
Average speed for network part   2 iteration       9 is                     :        27.10 km.hr

Total delay for the whole network of iteration   9 is                       :       504.20 veh.hrs
Total delay for network part   1 of iteration    9 is                       :       436.38 veh.hrs
Total delay for network part   2 of iteration    9 is                       :        67.82 veh.hrs

Total entrance delay for the whole network of iteration   9 is              :         0.00 veh.hrs
Total entrance delay for network part   1 of iteration    9 is              :         0.00 veh.hrs
Total entrance delay for network part   2 of iteration    9 is              :         0.00 veh.hrs


The smooth factor for the flows for iteration   9 and time period   1 is    :        0.1057
The smooth factor for the flows for iteration   9 and time period   2 is    :        0.1057
The smooth factor for the flows for iteration   9 and time period   3 is    :        0.1057
The smooth factor for the flows for iteration   9 and time period   4 is    :        0.1057
The smooth factor for the flows for iteration   9 and time period   5 is    :        0.1057
The smooth factor for the flows for iteration   9 and time period   6 is    :        0.1057
The smooth factor for the flows for iteration   9 and time period   7 is    :        0.1057

//LinkOutput (after the final iteration)
------------------------------------------------------------------------------------------------------
       period|      linknr|  link length|   density|   speed| std speed|    inflow|   outflow|   queue|
             |            |      (m)    |(veh/km.l)| (km/hr)|   (km/hr)|  (veh/hr)|  (veh/hr)|     (m)|
-------------|------------|-------------|----------|--------|----------|----------|----------|--------|
            1            1          2713     14.188   114.55       0.00    3405.00    3405.00        0  
            1            2           670     13.563   115.55       0.00    3255.00    3255.00        0  
            1            3          2045     14.808   113.52       0.10    3588.33    3595.17        0  
            1            4          1046     15.013   107.06       3.79    3928.50    3954.06        0  
            1            5           500     85.150    11.74       5.67     576.21     333.33      293  
            1            6          1654      9.785    76.31       6.91     655.15     576.21       20  
            1            7           500     20.658    19.10      10.21     394.85     333.33       59  
            1            8           715      4.936    79.78       0.00     394.85     394.85        0  
            1            9           702      2.143    32.29       0.00     150.00     150.00        0  
            1           11           999      7.500    69.52       0.00    1050.00    1050.00        0  
            1           12           570      2.143    69.90       0.00     150.00     150.00        0  
            1           13           400      9.359    29.55       0.00     655.15     655.15        0  
            1           14           400      5.641    28.49       0.00     394.85     394.85        0  
            2            1          2713     19.439    86.73       4.24    4190.00    4067.89        0  
            2            2           670     20.735    95.48      11.32    3874.27    3812.11       11  
            2            3          2045     76.643    37.39      23.82    4145.44    2522.67      802  
            2            4          1046     27.083    53.88      22.01    2856.00    2790.16       95  
            2            5           500    129.630    10.00       0.00     333.33     333.33      472  
            2            6          1654     55.361    32.84      10.24     805.90     333.33      534  
            2            7           500     49.264    10.37       1.19     443.80     333.33      135  
            2            8           715      5.317    79.74       0.10     451.60     443.80        0  
            2            9           702      3.998    31.44       0.33     193.61     187.23        0  
            2           11           999     12.963    64.56       4.77    1575.00    1509.68       17  
            2           12           570      2.660    69.87       0.02     187.23     185.63        0  
            2           13           400     95.715    13.71       6.29     985.93     805.90      210  
            2           14           400     18.792    25.35       4.93     523.76     451.60        9  
            3            1          2713     17.986   106.49       3.11    3875.00    3917.00        0  
            3            2           670     17.783   102.65      13.57    3715.19    3766.79        8  
            3            3          2045    120.522    18.49       0.61    4100.12    3950.67     1445  
            3            4          1046     22.752    85.00       0.00    4284.00    4284.00        0  
            3            5           500    129.630    10.00       0.00     333.33     333.33      472  
            3            6          1654    121.529    14.88       2.09     602.38     333.33     1400  
            3            7           500    124.683    10.00       0.00     410.74     333.33      406  
            3            8           715     33.925    50.13      22.90     612.37     410.74      141  
            3            9           702      4.504    31.25       0.10     201.81     201.81        0  
            3           11           999      9.855    63.99       4.06    1260.00    1289.69       18  
            3           12           570      2.709    69.86       0.00     201.81     202.34        0  
            3           13           400    124.967    10.00       0.00     613.30     602.38      349  
            3           14           400     53.136    14.11       2.53     676.39     612.37       88  
            4            1          2713     14.142   115.39       1.29    3250.00    3335.78        0  
            4            2           670     13.530   115.16       2.26    3231.34    3244.61        0  
            4            3          2045    113.868    17.72       0.34    3577.94    3950.67     1560  
            4            4          1046     22.752    85.00       0.00    4284.00    4284.00        0  
            4            5           500    129.630    10.00       0.00     333.33     333.33      472  
            4            6          1654    132.214    12.81       0.00     333.33     333.33     1626  
            4            7           500    129.630    10.00       0.00     333.33     333.33      468  
            4            8           715    117.156    15.10       2.47     483.71     333.33      599  
            4            9           702      1.074    33.16       0.43     104.43     114.62        0  
            4           11           999     26.430    40.62       8.16    1050.00     817.14      164  
            4           12           570      1.220    69.92       0.03     114.62     118.35        0  
            4           13           400    128.704    10.00       0.00     333.33     333.33      372  
            4           14           400     71.216    11.32       1.09     483.81     483.71      184  
            5            1          2713      7.834   118.46       0.44    2200.00    2340.00        0  
            5            2           670      9.265   118.29       0.88    2234.70    2258.03        0  
            5            3          2045    109.043    17.54       0.39    3166.67    3018.70     1591  
            5            4          1046     22.752    85.00       0.00    4284.00    4284.00        0  
            5            5           500    119.274    15.82       1.41    1244.59    1265.30      233  
            5            6          1654     98.045    20.70       5.34     802.90    1244.59      945  
            5            7           500    117.746    12.42       3.04     769.14     908.64      261  
            5            8           715     67.817    32.97      22.31     396.99     769.14      297  
            5            9           702      1.001    33.19       0.31     105.30     105.30        0  
            5           11           999     13.445    53.34      16.29     630.00     944.43       87  
            5           12           570      1.093    69.93       0.01     105.30     105.30        0  
            5           13           400    109.350    11.83       2.60     691.18     802.90      201  
            5           14           400     36.637    20.64      10.47     253.25     396.99       99  
            6            1          2713      1.519   119.47       0.14    1150.00    1286.71        0  
            6            2           670      4.879   119.43       0.29    1176.85    1200.18        0  
            6            3          2045     65.291    35.28      26.95    1359.60    3124.86      970  
            6            4          1046     22.059    86.31       6.15    4132.08    4284.00        0  
            6            5           500     62.376    51.36      22.53     774.83    1007.22      150  
            6            6          1654     18.412    65.14      19.06     364.73     774.83      105  
            6            7           500      2.186    76.01      10.27      40.51     159.42        6  
            6            8           715      0.314    79.98       0.00      39.58      40.51        0  
            6            9           702      1.168    33.10       0.57     109.86     109.86        0  
            6           11           999      0.876    69.88       0.02     315.00     322.00        0  
            6           12           570      1.153    69.93       0.02     109.86     109.86        0  
            6           13           400     11.822    33.24       4.71     283.13     364.73        6  
            6           14           400      0.542    34.00       0.09      38.87      39.58        0  
            7            1          2713      1.177   119.49       0.00    1150.00    1150.00        0  
            7            2           670      4.353   119.55       0.00    1050.00    1050.00        0  
            7            3          2045      1.631   119.53       0.01    1112.03    1108.83        0  
            7            4          1046      3.704   119.23       0.91    1363.85    1370.96        0  
            7            5           500      2.826    79.54       0.03     254.38     255.02        0  
            7            6          1654      3.058    79.87       0.01     251.17     254.38        0  
            7            7           500      0.777    79.90       0.02      62.85      62.03        0  
            7            8           715      0.763    79.97       0.00      64.35      62.85        0  
            7            9           702      0.791    33.30       0.00     100.00     100.00        0  
            7           11           999      0.876    69.88       0.00     315.00     315.00        0  
            7           12           570      0.975    69.93       0.00     100.00     100.00        0  
            7           13           400      6.364    35.51       0.08     248.62     251.17        0  
            7           14           400      1.744    33.62       0.09      66.38      64.35        0  
//End---------------------------------------------------------------------------


The results of the final iteration for the flows, travel times and green times are: 


//RouteFlows (in veh/hr)
------------------------
 Route         1         2         3         4         5         6         7
     1  3255.000  3990.000  3675.000  3150.000  2100.000  1050.000  1050.000
     2   150.000   200.000   200.000   100.000   100.000   100.000   100.000
     3   655.146  1219.252   861.201   918.160   562.965   276.766   247.976
     4   394.854   355.748   398.799   131.840    67.035    38.234    67.024
//End-------------------


//RouteTravelTime (in minutes)
------------------------------
 Route         1         2         3         4         5         6         7
     1      3.54      8.00      9.40      9.41      9.48      6.76      3.25
     2      3.21      3.67      3.40      3.18      3.14      3.13      3.12
     3      6.95     10.68     14.25     14.55      9.91      4.51      3.68
     4      6.64     11.72     14.54     17.15     14.31      7.26      4.04
//End-------------------------


//RouteDelay (in minutes)
-------------------------
 Route         1         2         3         4         5         6         7
     1      0.31      4.76      6.17      6.18      6.25      3.52      0.01
     2      0.77      1.22      0.95      0.73      0.69      0.68      0.67
     3      3.61      7.34     10.91     11.21      6.57      1.17      0.34
     4      2.99      8.06     10.88     13.49     10.65      3.61      0.38
//End--------------------


//RouteSpeed (in km/hr)
-----------------------
 Route   Length         1         2         3         4         5         6         7
     1     6.47    109.64     48.56     41.30     41.26     40.96     57.50    119.49
     2     3.98     74.37     65.14     70.32     75.27     76.26     76.49     76.73
     3     4.60     39.73     25.85     19.37     18.96     27.84     61.21     75.01
     4     5.71     51.51     29.21     23.55     19.96     23.92     47.12     84.81
//End------------------


//RoutePartFlow (in veh/hr)
---------------------------
RoutePart         1         2         3         4         5         6         7
        9  3255.000  3990.000  3675.000  3150.000  2100.000  1050.000  1050.000
       10     0.000     0.000     0.000     0.000     0.000     0.000     0.000
//End----------------------


//RoutePartTravelTime (in minutes)
----------------------------------
RoutePart         1         2         3         4         5         6         7
        9      3.54      8.00      9.40      9.41      9.48      6.76      3.25
       10      8.04     13.28     14.79     16.33     14.07      7.91      5.09
//End-----------------------------


//RoutePartDelay (in minutes)
-----------------------------
RoutePart         1         2         3         4         5         6         7
        9      0.31      4.76      6.17      6.18      6.25      3.52      0.01
       10      3.62      8.86     10.37     11.91      9.66      3.49      0.68
//End------------------------


//RoutePartSpeed (in km/hr)
---------------------------
RoutePart         1         2         3         4         5         6         7
        9    109.64     48.56     41.30     41.26     40.96     57.50    119.49
       10     57.63     34.89     31.33     28.38     32.92     58.59     90.99
//End----------------------


//SignalTimings (in seconds)
----------------------------
 Ctr       Sig         1         2         3         4         5         6         7
   1         1       2.0       2.0       2.0       2.0       7.6      12.0      12.0
   1     Cycle      12.0      12.0      12.0      12.0      12.0      12.0      12.0
   2         1       2.0       2.0       2.0       2.0       5.5       9.4      12.0
   2     Cycle      12.0      12.0      12.0      12.0      12.0      12.0      12.0
   3         8      40.0      40.0      40.0      40.0      40.0      40.0      40.0
   3         9      33.0      33.0      33.0      33.0      33.0      33.0      33.0
   3        11      14.0      14.0      14.0      14.0      14.0      14.0      14.0
   3     Cycle      97.0      97.0      97.0      97.0      97.0      97.0      97.0
//End-----------------------


//Total distance travelled (veh.km)
-----------------------------------
NetType         1         2         3         4         5         6         7      Totals
      1   6107.33   6826.45   6876.85   5961.01   5104.79   2915.70   2004.25    35796.39
      2    486.96    646.65    549.49    420.28    440.85    242.66    173.77     2960.66
//End------------------------------


//Total time spent (veh.hrs)
----------------------------
NetType         1         2         3         4         5         6         7      Totals
      1     58.31    147.37    182.45    161.06    149.46     50.63     17.29      766.56
      2     15.21     22.19     21.73     19.30     21.66      5.17      3.15      108.42
//End-----------------------


//Average speed (km/hr)
-----------------------
NetType         1         2         3         4         5         6         7      Totals
      1    104.73     46.32     37.69     37.01     34.15     57.59    115.93       46.70
      2     32.01     29.14     25.29     21.78     20.35     46.91     55.10       27.31
//End------------------


//Total tolls (euros)
---------------------
NetType         1         2         3         4         5         6         7      Totals
      1    610.73    682.64    687.69    596.10    510.48    291.57    200.43     3579.64
      2     48.70     64.67     54.95     42.03     44.08     24.27     17.38      296.07
//End----------------


//Total delay (veh.hrs)
-----------------------
NetType         1         2         3         4         5         6         7      Totals
      1      5.79     88.53    123.43    110.27    104.84     25.65      0.07      458.58
      2      8.38     13.03     13.95     13.37     15.64      1.88      0.73       66.98
//End------------------


//Entrance delays (veh.hrs)
---------------------------
 Origin         1         2         3         4         5         6         7      Totals
      1      0.00      0.00      0.00      0.00      0.00      0.00      0.00        0.00
     10      0.00      0.00      0.00      0.00      0.00      0.00      0.00        0.00
//End----------------------


//Entrance delays (veh.hrs)
---------------------------
NetType         1         2         3         4         5         6         7      Totals
      1      0.00      0.00      0.00      0.00      0.00      0.00      0.00        0.00
      2      0.00      0.00      0.00      0.00      0.00      0.00      0.00        0.00
//End----------------------


//Number of vehicles (veh)
--------------------------
                1         2         3         4         5         6         7      Totals
Demand       1114      1441      1284      1075       708       366       366        6354
Departed     1114      1441      1284      1075       707       366       366        6354
Arrived      1026       744      1122      1101      1097      1098       368        6556
//End---------------------


//Vehicles in network (veh)
---------------------------
  Start         1         2         3         4         5         6         7
    242       330      1027      1189      1164       774        42        40
//End----------------------


//Vehicles in origins (veh)
---------------------------
 Origin         1         2         3         4         5         6         7      Totals
      1         0         0         0         0         0         0         0           0
     10         0         0         0         0         0         0         0           0
 Totals         0         0         0         0         0         0         0           0
//End----------------------


Total number of iterations is  :           9

Total demand (number of vehicles) is    :        6354
Total number of departed vehicles is    :        6354
Total number of arrived vehicles is     :        6556

Total distance travelled for the whole network for the final iteration is :     38757.05 veh.km
Total distance travelled for network part   1 for the final iteration is  :     35796.39 veh.km
Total distance travelled for network part   2 for the final iteration is  :      2960.66 veh.km

Total time spent for the whole network for the final iteration is         :       874.98 veh.hrs
Total time spent for network part   1 for the final iteration is          :       766.56 veh.hrs
Total time spent for network part   2 for the final iteration is          :       108.42 veh.hrs

Average speed for the whole network for the final iteration is            :        44.29 km.hr
Average speed for network part   1 for the final iteration is             :        46.70 km.hr
Average speed for network part   2 for the final iteration is             :        27.31 km.hr

Total toll for the whole network for the final iteration is               :      3875.70 Euro
Total toll for network part   1 for the final iteration is                :      3579.64 Euro
Total toll for network part   2 for the final iteration is                :       296.07 Euro

Total delay for the whole network for the final iteration is              :       525.56 veh.hrs
Total delay for network part   1 for the final iteration is               :       458.58 veh.hrs
Total delay for network part   2 for the final iteration is               :        66.98 veh.hrs

Total entrance delay for the whole network for the final iteration is     :         0.00 veh.hrs
Total entrance delay for network part   1 for the final iteration is      :         0.00 veh.hrs
Total entrance delay for network part   2 for the final iteration is      :         0.00 veh.hrs


//NetworkOutput - Final Iteration
------------------------------------------------------------------------------------------
|  Network  |  Total number  |  Total distance  |  Total time  |     Total    |  Average  |
|   part    |  of vehicles   |    travelled     |     spent    |     delay    |   speed   |
|           |                |     (veh.km)     |   (veh.hrs)  |   (veh.hrs)  |  (km/hr)  |
------------------------------------------------------------------------------------------
|           |           6354 |         38757.05 |       874.98 |       525.56 |     44.29 |
------------------------------------------------------------------------------------------
|     1     |                |         35796.39 |       766.56 |       458.58 |     46.70 |
|     2     |                |          2960.66 |       108.42 |        66.98 |     27.31 |
------------------------------------------------------------------------------------------

//NetworkOutput - Sum of Iterations
-------------------------------------------------------------
|  Network  |  Total distance  |  Total time  |     Total    |
|   part    |    travelled     |     spent    |     delay    |
|           |     (veh.km)     |   (veh.hrs)  |   (veh.hrs)  |
-------------------------------------------------------------
|           |        387725.20 |      8630.12 |      5135.20 |
-------------------------------------------------------------
|     1     |        358182.80 |      7552.68 |      4471.31 |
|     2     |         29542.40 |      1077.44 |       663.89 |
-------------------------------------------------------------

//NetworkOutput - Average of Iterations
-------------------------------------------------------------
|  Network  |  Total distance  |  Total time  |     Total    |
|   part    |    travelled     |     spent    |     delay    |
|           |     (veh.km)     |   (veh.hrs)  |   (veh.hrs)  |
-------------------------------------------------------------
|           |         38772.52 |       863.01 |       513.52 |
-------------------------------------------------------------
|     1     |         35818.28 |       755.27 |       447.13 |
|     2     |          2954.24 |       107.74 |        66.39 |
-------------------------------------------------------------


The results of the final iteration for the emissions are: 


//EmissionsOutput
----------------------------------------------------------------------------------------
|  Network  |    Emission   |   Emission   |   Emission   |   Emission   |   Emission   |
|   part    |          CO   |        CO2   |         HC   |        NOx   |         PM   |
|           |        (gr)   |       (kg)   |       (gr)   |       (gr)   |       (gr)   |
----------------------------------------------------------------------------------------
|           |      76696.94 |     10507.87 |       801.87 |     35233.01 |       573.01 |
----------------------------------------------------------------------------------------
|     1     |      66012.08 |      9371.47 |       690.45 |     31026.96 |       517.03 |
|     2     |      10684.86 |      1136.41 |       111.42 |      4206.06 |        55.97 |
----------------------------------------------------------------------------------------


Date and time of ending the run is: 18-Jul-2025 16:37:54

Total time of the run is:     8.86 seconds (is     0.15 minutes)
